Gas oven purchase

* Ovens must be natural gas fired
* Must have computer controls with digital time and temp readouts
* Roast and hold cycle
* Programable menu selection
* Need two ovens with a stacking kit, no casters
* Stainless steel exterior
* Porcelain enamel interior
* 50,000 BTU burner per section
* Independently operated stainless steel doors with double pain windows
* Five oven racks per section
* One year parts and labor
* Must be able to provide onsite service within 48 hours of service call
* Cool down function for faster cool down
* Electronic spark ignitors
* 120 volt with two speed blower motor and 6’ cord
* Interior oven lights
* Need to have positive rack stops with eleven rack guides
* Dimensions 40 ¼” w X 41 1/8”d (include motor & door handles) 37 ¾ d includes motor only) x 70 h on 8” legs.