Bid requirements for ligature resistant radiator covers

Must be ligature resistant covers

Must be 14 gauge cold rolled steel

Must be coated with primer then finished with powder coat

Must have removable access panel with anti-ligature locks

Must cover all exposed piping

Must cover completely to the floor

Must be manufacturer installed

Installer must make all adjustment to wall and cover to make cover safe