Civil Commitment Unit for Sexual Offenders

1251 W Cedar Loop

Cherokee, IA 51012

BID 406JL1929910

DETENTION HOLLOW METAL DOORS

2 – 2” X 3’0” X 7’0” Hollow Metal Doors

Detention/Security grade doors

20 minute fire rating

Mortised for Yale 8800 series locks

Must have pass through door and security window with metal meshing (as shown)

\*\*\*existing door photos attached for reference purposes\*\*\*

\*\*\*\*New doors to increase height of pass door\*\*\*\*

Doors to be installed by Contractor

Removal of existing hardware from current doors by Contractor

Existing hardware to be installed on new doors by Contractor

New doors to be painted gray to match existing frames by Contractor

Site visit required by Contractor to verify all measurements of existing frames for door size accuracy prior to submission of shop drawing

Shop drawing must be provided to Plant manager for review and approval prior to production of new doors